###### ZTP

***Objective:***

Objective is to install SAOS 10.x with ZTP process. Network based ZTP process is useful when we want to ensure the same version of software is automatically installed on multiple nodes in the network. ZTP only allowed over VLAN 127, and untagged is not supported.

***Procedure:***

* Ensure you have DHCP environment setup is been done with either of
  + Option 66/67 to provide tftp server and filename of Command File
  + Option 125 to provide URL of Command Fil
* Ensure that the image you want to download is located on an HTTP/TFTP server
* Verify that the command file is located at the TFTP server and the config file is supplied
* Start the node if it is the first time it is being powered up
* Once the device boots up, Login to UI container using the management IP you checked in the previous step (default login/passwd displayed below):

ssh [diag@x.x.x.x](mailto:diag@x.x.x.x)

username: diag password: ciena123

Test Case Results:

Passed: Yes No Verified by Date/Time Comments