###### Low Latency Bypass (currently only available on 5162)

***Objective:***

Enable low latency bypass. LLBP can only be enabled on 5162. This feature enable a specific internal datapath to support performance and scale for features such as IP BFD and CFM.

***Procedure:***

* Unbind the logical port 40.
  + no logical-ports logical-port 40 binding
* Activate interface 40’s LLBP.
  + oc-if:interfaces interface 40 config offload-activate true
* This will enable a lower latency internal data path.

Test Case Results:

Passed: Yes No Verified by Date/Time Comments