###### Verify USB-based installation of SAOS 10.x

***Objective:***

Objective is to install SAOS 10.x on a system using USB-based method.

***Procedure:***

* Ensure that the format of your USB stick is FAT32 formatted.
* Ensure that the image you want is on the USB stick
* Ensure that the image is named “**onie-installer**”. This is important. Currently, the load name cannot be named anything else.
* Start the node if it is the first time it is being powered up, or follow the following steps otherwise
* Login to UI container using the management IP you checked in the previous step:

ssh [diag@x.x.x.x](mailto:diag@x.x.x.x)

username: diag password: ciena123

When ONIE comes up it will try to find the resource for ZTP. Wait for the installation to complete from here.

Test Case Results:

Passed: Yes No Verified by Date/Time Comments