###### DHCPv6 Client Setup

***Objective:***

Ensure that with DHCPv6 client enabled, the interface will acquire an IPv6 address automatically. **Only stateful DHCPv6 (no SLAAC) is currently supported.**

***Procedure:***

* Dual IPv4 and IPv6 stack on mgmt. interfaces are supported as of 10.3 and onwards. Enable DHCPv6 client on mgmtbr0. Ensure that :
  + config
  + dhcpv6-client client mgmtbr0 admin-enable true
* Configure IPv4 static IP on the mgmtbr0 as well.
  + dhcp-client client mgmtbr0 admin-enable false
  + oc-if:interfaces interface mgmtbr0 ipv4 address address x.x.x.x config ip x.x.x.x prefix-length 20
  + rib vrf default ipv4 x.x.x.x/8 next-hop x.x.x.x description "lab default"


Ex:

dhcp-client client mgmtbr0 admin-enable false

oc-if:interfaces interface mgmtbr0 ipv4 address address 10.181.36.85 config ip 10.181.36.85 prefix-length 20

rib vrf default ipv4 10.0.0.0/8 next-hop 10.181.32.1 description "lab default"

* Display the IPv6 and IPv4 interfaces on the node.
  + 5170-0037> show ipv6 interfaces brief



* + 5170-0037> show ip interfaces brief

A screenshot of a computer

Description automatically generated with medium confidence

5170-0037> show dhcpv6

+-------- DHCPV6 CLIENT CONFIGURATION +

| Name | Value |

+ + +

| Interface Name | mgmtbr0 |

| Admin State | Enabled |

| Rapid Commit | Enabled |

| Requested Preferred Lifetime (s) | 0 |

| Requested Valid Lifetime (s) | 0 |

| Option | |

| DNS Server List | Enabled |

| Domain Search List | Enabled |

| Posix Time Zone | Disabled |

| TZDB Time Zone | Enabled |

| NTP Server | Enabled |

| Bootfile URL | Enabled |

+ + +

| Interface Name | remote |

| Admin State | Enabled |

| Rapid Commit | Enabled |

| Requested Preferred Lifetime (s) | 0 |

| Requested Valid Lifetime (s) | 0 |

| Option | |

| DNS Server List | Enabled |

| Domain Search List | Enabled |

| Posix Time Zone | Disabled |

| TZDB Time Zone | Enabled |

| NTP Server | Enabled |

| Bootfile URL | Enabled |

+ + +

+ DHCPV6 CLIENT STATE +

| Name | Value |

+ + +

| Interface Name | remote |

| Oper State | Enabled |

| DHCPv6 State | preinit |

| Config State | stateful |

| Renewal (T1) Time (s) | |

| Renewal (T1) Time Remaining (s) | |

| Rebinding (T2) Time (s) | |

| Rebinding (T2) Time Remaining (s) | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| |  |  |  | | Preferred Lifetime (s) Preferred Lifetime Remaining Valid Lifetime (s)  Valid Lifetime Remaining (s) | (s) | |  |  |  | |  | |  |  |  | |
| |  |  |  |  |  |  |  |  +  | | DHCPv6 Server DUID Option Value  DNS Server List Domain Search List Posix Time Zone TZDB Time Zone  NTP servers Boot File URL  Interface Name |  | |  |  |  |  |  |  |  |  +  | | mgmtbr0 | |  |  |  |  |  |  |  |  +  | |
| **|**  **|**  **|**  | | **Oper State DHCPv6 State Config State**  Renewal (T1) Time (s) |  | **|**  **|**  **|**  | | **Enabled bound stateful**  302400 | **|**  **|**  **|**  | |
| | | Renewal (T1) Time Remaining | (s) | | | 241733 | | |
| | | Rebinding (T2) Time (s) | | | | 453600 | | |
| | | Rebinding (T2) Time Remaining (s) | | | | 392933 | | |
| | | Preferred Lifetime (s) | | | | 604800 | | |
| | | Preferred Lifetime Remaining (s) | | | | 544133 | | |
| | | Valid Lifetime (s) | | | | 604800 | | |
| | | Valid Lifetime Remaining (s) | | | | 544133 | | |
| |  |  |  |  |  |  |  |  + | DHCPv6 Server DUID Option Value  DNS Server List Domain Search List Posix Time Zone TZDB Time Zone  NTP servers Boot File URL | | |  |  |  |  |  |  |  |  + | 0:1:0:1:25:22:d:24:0:0:5e:0:1:81 | |  |  |  |  |  |  |  |  + |

Test Case Results:

Passed: Yes No Verified by Date/Time Comments