###### FRU – Filler Mismatch Alarm Disable

***Objective:***

* + - * Objective is to disable FRU filler mismatch alarm. This testcase is only applicable to 5171, 8110, 8114, and 8180.

Pre-requisites:

* + - * Fill module in device.

***Procedure:***

* + - * Have a filler module in the device. Then pre-configure the same slot to an actual FRU module type**.** Ex:

config

components component 'slot2' properties property 'fru-type' config name "fru-type" value qsfp28

* + - * Check alarms to see if filler mismatch alarm is raised.

show alarm list active-alarms alarm-type all

* + - * Configure filler mismatch alarm as disabled

config

components component slot2 properties property filler-mismatch- alarm config name filler-mismatch-alarm value **disabled**

* + - * Verify alarms again to ensure that the filler mismatch alarm is cleared.

Test Case Results:

Passed: Yes No Verified by Date/Time Comments