###### Configure CFP2-DCO ports

***Objective:***

Configure CFP2-DCO ports.

***Procedure:***

* ***Prerequisites –*** device must have valid license and FRU should be in UP state
* Set frequency of the port

>config

#ptps ptp <slot/port> properties transmitter frequency value

<0.0 | 186087.5 .. 190956.2 | 191100.0 .. 196150.0 >

* Verify the port status

5171-A> show logical-ports logical-port 1/1.1

+---- LOGICAL PORT +

| KEY | VALUE |

+ + +

| Name | 1/1.1 |

| Ettp | 1/1.1 |

| Admin State | enable |

| MTU | 1526 |

| Description | 1/1.1 |

+ + +

+------- LOGICAL PORT STATE +

| KEY | VALUE |

+ + +

| Name | 1/1.1 |

| Index | 41 |

| Mac Address | 20:80:58:81:87:b2 |

| Oper State | Up |

+ + +

Test Case Results:

Passed: Yes No Verified by Date/Time Comments