

5.11.4 Configurable BFD session Parameters

admin-down Is the BFD session administratively down.

desired-min-tx-interval Desired minimum transmit interval of control packets in microseconds.

Range 10ms – 10 seconds

local-multiplier Multiplier transmitted by local system. Range 3 - 50 required-min-rx-interval Required minimum receive interval of control packets in

microseconds. Range 10ms – 10 seconds

Objective:

**To Disable BFD session on MPLS TP Tunnel Procedure:**

* Go to the configuration terminal config
* Enter the following command to Disable BFD session on primary ingress Tunnel

tp-corouted-tunnels tunnel tunnel\_150 1.1.1.1 3.3.3.3 tunnel-type static-ingress-corouted

bfd-cfg-parms “admin-down true”

exit

* Enter the following command to Disable BFD session on primary egress Tunnel tp-corouted-tunnels tunnel tunnel\_150 1.1.1.1 3.3.3.3

tunnel-type static-egress-corouted bfd-cfg-parms “admin-down true” exit

Test Case Results:

Passed: Yes No Verified by Date/Time Comments