###### L2VPN OAM

***Objective:***

Objective is to verify connectivity of L2VPN created between PE nodes using ping comman



**PE-1**

**PE-2**

P1 P2

Loopback

Loopback

***Procedure:***

* The L2VPN ping on pseudowire PW1 between PE nodes in above topology diagram can be triggered using the command :-
  + ping mpls pseudowire pseudowire-name PW1
* interval (Send delay between requests in milliseconds, default is set to 1000 msec, range is 1000 to 20000 msec)
* repeat-count (Number of echo requests to be sent out, default is set to 5, range is 5 to 200)
* timeout (Timeout value in seconds, default is set to 2 sec, range is 1 to 60 sec)
* ttl (Time-to-live value, default is set to 255, range is 1 to 255)

Test Case Results:

Passed: Yes No Verified by Date/Time Comments