Ingress Metering – QoS Flow only

***Objective:***

Verify that traffic must adhere to QoS flow meter profile.

***Procedure:***

* In previous testcases, the QoS flow (qf1-cos8-cos16) with classification of internal CoS 8 or 16 metered to 2G and also a catch call QoS flow (qos-catchall) metered to 2G was also created.
* In previous testcases, a 4G meter profile was also added onto the parent flow point.
* Send traffic from traffic generator:
  + Send 2G traffic that would classify to QoS flow qf1-cos8-cos16.
    - **Result**: This traffic stream will be metered to 2G.
  + Also send 4G traffic that would classify to the catch all QoS flow.
    - **Result**: this traffic stream will be metered to 2G of traffic as well. Packets will be discarded.

Test Case Results:

Passed: Yes No Verified by Date/Time Comments