###### ONU Configuration

***Objective:***

The objective of this test is to configure an ONU. The serial number of each connected ONU is required for this step. The user is still required to configure the ONU data link which establishes a channel between ONU and uOLT.

***Procedure:***

1. Enter the serial number of each connected ONU.

pon-ctrl onus onu ONU\_1 OLT\_1 serial-number ALPHe30cae24 pon-ctrl onus onu ONU\_2 OLT\_1 serial-number ALPHe3d367c7 pon-ctrl onus onu ONU\_3 OLT\_1 serial-number ALPHe3d36588

***Expected Results:***

5170\_PON> show pon-ctrl olts olt OLT\_1 onus

+ ONUS +

| Name | Serial Number | Oper State | ONU-ID | Number of Links |

+ + + + + +

| ONU\_1 | ALPHE30CAE24 | Registered | 3 | 2 |

| ONU\_2 | ALPHE3D367C7 | Registered | 2 | 2 |

| ONU\_3 | ALPHE3D36588 | Registered | 1 | 1 |

+ + + + + +

Test Case Results:

Passed: Yes No Verified by Date/Time Comments