###### Traffic flows to ONUs Via uOLT and Vice versa

When configuring a test set to send traffic, ensure that that source and destination MAC addresses are configured accordingly. Traffic flows to a data link based on MAC learning as multiple data links can be attached to the same network. Start the upstream traffic first so the uOLT can learn the source MAC to determine the correct data link to send downstream frames.