Register ONUs

***Objective:***

The objective of this test is to register and configure connected ONUs.

ONU Registration

***Procedure:***

When an uOLT is active and ONUs are connected, they automatically register with the uOLT and the ONU count is displayed per uOLT.

5170\_PON> show pon-ctrl olts

+ OLTS +

| Name | MAC Address | Oper State | Registered ONUs |

+ + + + +

| OLT\_1 | 70:B3:D5:52:32:12 | Active | 1 |

+ + + + +