###### ONU and UNI Port Configuration

***Objective:***

The objective of this test is to configure an ONU. The serial number of each connected ONU is required for this step. The user is still required to configure the ONU data link which establishes a channel between ONU and uOLT.

***Procedure:***

Enter the serial number of each connected ONU.

pon-ctrl onus onu ONU\_2 OLT\_1 serial-number CIEN00001642 UNI Port config:

pon-ctrl onus onu ONU\_2 OLT\_1 uni-ports uni-port 1 admin-state enabled