###### Configuration of Service Activation Test Reflector.

***Objective:***

Objective is to configure of service activation test reflector.

***Procedure:***

* Setup the Fowarding Domains and classifiers and flow points in CLI:
  + Enter “config”

fds fd fd-1G mode vpws

classifiers classifier vlan\_100 filter-entry vtag-stack vtags 1 vlan-id 100

fps fp fp\_NNI logical-port 1 fd-name fd-1G classifier- list vlan\_100

fps fp fp\_PUT logical-port 2 fd-name fd-1G classifier- list vlan\_100

* Setup the SAT configuration on the flow point provisioned. The SAT is only running on VLAN 100 in this example:

sat entity ref port 2 role reflector reflection-level l2- to-l4

sat test-instance test-1 flow-point-id fp\_PUT c-vid 100

* Enable the SAT globally as well as the test instance. sat sat-global admin-state enabled sat entity ref admin-state enabled

sat test-instance test-1 admin-state enabled

* The reflector is now active. Once the remote generator is activated, reflector test will reflect packets.

Test Case Results:

Passed: Yes No Verified by Date/Time Comments