###### User Configurable Reg-Id

A device is licensed with license server using 40 characters registration id by default.

What new we are getting in saos 10.7.1 is that we will be able to change the registration ID to any customized value on the device which is used for licensing.

The main advantage of this feature is that we will be easily able to identify the clients connected to license server.

***Objective:***

Objective is to change the Reg-Id of the node to the customized value.

***Procedure:***

Below is the command with which we can configure the customized reg-id on the node. Max characters allowed under this section is 30.

Text

Description automatically generated

It can be noted that once the customzed reg id is defined, the 8 chars device Id is automatically appended to the reg-id. This is the hash value of chassis serial no and is basically added to keep the reg-Id unique.

In case we unconfigure the customized reg id on the device,the device rolls back to its previuos 40 chars reg id.

One thing worth noting here is that this functionality is only applicable when licensing using server and will not be applicable when licensing using file.

Test Case Results:

Passed: Yes No Verified by Date/Time Comments