###### Verify Manual network-based installation

***Objective:***

Objective is to install SAOS 10.x on a system, using the manual network-based installation.

***Procedure:***

* Login to system console port.
* When ONIE comes up it will try to find the resource for ZTP. If you want to specify the location of the installer file manually, which is different from what it might fetch from network installer, you should stop it:

ONIE:/ # onie-discovery-stop

* Then proceed with the manual installation from the installer file from http, tftp or ftp server.

ONIE:/ # onie-nos-install <http://x.x.x.x/installer.bin> ONIE:/ # onie-nos-install tftp://x.x.x.x/installer.bin ONIE:/ # onie-nos-install ftp://x.x.x.x/installer.bin

Replace x.x.x.x with IP address or the URL of where the image is residing. Here is an example:

ONIE:/ # onie-nos-install <http://x.x.x.x/valimar-> snapshot/17-12-00-0141/meta-onie-installer-dnx/meta\_01-00- 00-0181-core.bin

Test Case Results:

Passed: Yes No Verified by Date/Time Comments