###### Verify System Power Cycle will maintain the configuration

***Objective:***

To verify that SAOS 10.x on sytem maintains configuration and operation following a disruption to power.

***Procedure:***

* Login to UI container using the management IP you checked in the previous step:

ssh [diag@x.x.x.x](mailto:diag@x.x.x.x)

username: diag password: ciena123

* Then issue the reboot command below or power cycle the node.
  + system restart
* Once powered up verify that device can be reachable by management network, and login is re-enabled.
* Login to the box and confirm configuration is still in place.

Test Case Results:

Passed: Yes No Verified by Date/Time Comments