###### Test payload calculation mode in ingress metering with traffic

***Objective:***

Objective is to verify ingress metering bandwidth calculation mode application

***Procedure:***

* Follow the steps 3.3.1 and 3.3.3 to create a meter-profile and attaching it to an ingress flow point
* Run Ixia Traffic and confirm seeing the eir rate
* Change bandwidth calculation mode setting using step 3.3.2
* Confirm a slight increase in the received traffic
* Change back the bandwidth calculation mode using the following commands

bw-calculation-mode iqos-bw-calculation-mode transport bw-calculation-mode eqos-bw-calculation-mode transport

* Confirm a slight decrease in the received traffic

Test Case Results:

Passed: Yes No Verified by Date/Time Comments