###### Verify EQoS with traffic

***Objective:***

Objective is to verify effect of EQoS setup on egress traffic

***Procedure:***

* Run traffic on the node at port rate
* Follow the steps previous testcases to set up EQoS
* Restart traffic and confirm the cir/eir limits on the egress traffic
* Capture egress traffic and confirm packet flows received in the specified queue weight they are assigned to

Test Case Results:

Passed: Yes No Verified by Date/Time Comments