###### Create SLA Profile

***Objective:***

The objective of this test is to create a SLA profile. The SLA profile controls the bandwidth allocated to an ONU (upstream and downstream).

***Procedure:***

Configure upstream and downstream SLA parameters. pon-ctrl sla-profiles sla-profile SLA\_1

up-fixed-rate 0

up-guaranteed-rate 128

up-guaranteed-max-burst 409600

up-best-effort-rate 10000000

up-best-effort-max-burst 409600

up-priority 1

up-service-limit 128

up-min-grant-period 0

up-max-grant-period 10

down-guaranteed-rate 128

down-guaranteed-max-burst 262144

down-best-effort-rate 10000000

down-best-effort-max-burst 245760

exit exit exit