NNI Interface Configuration

***Procedure:***

pon-ctrl olts olt OLT\_1 nni-networks nni-network NNI\_Network\_1 match-stag 0

match-ctag-1 200

match-ctag-2 65535 tag-action none

exit exit exit exit exit